#
# Automatically generated file; DO NOT EDIT.
# misc/config System Configuration
#
CONFIG_SUBSYSTEM_TYPE_LINUX=y
CONFIG_SYSTEM_ZYNQ=y

#
# Linux Components Selection
#
CONFIG_SUBSYSTEM_COMPONENT_DEVICE__TREE_NAME_DEVICE__TREE__GENERATOR=y
CONFIG_SUBSYSTEM_COMPONENT_BOOTLOADER_AUTO_FSBL=y
CONFIG_SUBSYSTEM_COMPONENT_BOOTLOADER_NAME_ZYNQ_FSBL=y
CONFIG_SUBSYSTEM_COMPONENT_BOOTLOADER_AUTO_PS_INIT=y
CONFIG_SUBSYSTEM_COMPONENT_U__BOOT_NAME_U__BOOT__XLNX=y
# CONFIG_SUBSYSTEM_COMPONENT_U__BOOT_NAME_REMOTE is not set
# CONFIG_SUBSYSTEM_COMPONENT_U__BOOT_NAME_EXT__LOCAL__SRC is not set
CONFIG_SUBSYSTEM_COMPONENT_LINUX__KERNEL_NAME_LINUX__XLNX=y
# CONFIG_SUBSYSTEM_COMPONENT_LINUX__KERNEL_NAME_REMOTE is not set
# CONFIG_SUBSYSTEM_COMPONENT_LINUX__KERNEL_NAME_EXT__LOCAL__SRC is not set

#
# Auto Config Settings
#
CONFIG_SUBSYSTEM_AUTOCONFIG_DEVICE__TREE=y
# CONFIG_SUBSYSTEM_DEVICE_TREE_MANUAL_INCLUDE is not set
CONFIG_SUBSYSTEM_HARDWARE_AUTO=y
CONFIG_SUBSYSTEM_PROCESSOR0_IP_NAME="ps7_cortexa9_0"
CONFIG_SUBSYSTEM_PROCESSOR_ps7_cortexa9_0_SELECT=y
CONFIG_SUBSYSTEM_ARCH_ARM=y

#
# Memory Settings
#
CONFIG_SUBSYSTEM_MEMORY_PS7_DDR_0_BANKLESS_SELECT=y
# CONFIG_SUBSYSTEM_MEMORY_MANUAL_SELECT is not set
CONFIG_SUBSYSTEM_MEMORY_PS7_DDR_0_BANKLESS_BASEADDR=0x0
CONFIG_SUBSYSTEM_MEMORY_PS7_DDR_0_BANKLESS_SIZE=0x20000000
CONFIG_SUBSYSTEM_MEMORY_PS7_DDR_0_BANKLESS_KERNEL_BASEADDR=0x0
CONFIG_SUBSYSTEM_MEMORY_PS7_DDR_0_BANKLESS_U__BOOT_TEXTBASE_OFFSET=0x400000
CONFIG_SUBSYSTEM_MEMORY_IP_NAME="PS7_DDR_0"

#
# Serial Settings
#
CONFIG_SUBSYSTEM_FSBL_SERIAL_PS7_UART_0_SELECT=y
# CONFIG_SUBSYSTEM_FSBL_SERIAL_MANUAL_SELECT is not set
CONFIG_SUBSYSTEM_SERIAL_PS7_UART_0_SELECT=y
# CONFIG_SUBSYSTEM_SERIAL_MANUAL_SELECT is not set
# CONFIG_SUBSYSTEM_SERIAL_PS7_UART_0_BAUDRATE_600 is not set
# CONFIG_SUBSYSTEM_SERIAL_PS7_UART_0_BAUDRATE_9600 is not set
# CONFIG_SUBSYSTEM_SERIAL_PS7_UART_0_BAUDRATE_28800 is not set
CONFIG_SUBSYSTEM_SERIAL_PS7_UART_0_BAUDRATE_115200=y
# CONFIG_SUBSYSTEM_SERIAL_PS7_UART_0_BAUDRATE_230400 is not set
# CONFIG_SUBSYSTEM_SERIAL_PS7_UART_0_BAUDRATE_460800 is not set
# CONFIG_SUBSYSTEM_SERIAL_PS7_UART_0_BAUDRATE_921600 is not set
CONFIG_SUBSYSTEM_SERIAL_FSBL_IP_NAME="ps7_uart_0"
CONFIG_SUBSYSTEM_SERIAL_IP_NAME="ps7_uart_0"

#
# Ethernet Settings
#
CONFIG_SUBSYSTEM_ETHERNET_PS7_ETHERNET_0_SELECT=y
# CONFIG_SUBSYSTEM_ETHERNET_MANUAL_SELECT is not set
# CONFIG_SUBSYSTEM_ETHERNET_PS7_ETHERNET_0_MAC_AUTO is not set
CONFIG_SUBSYSTEM_ETHERNET_PS7_ETHERNET_0_MAC="00:0a:35:00:1e:53"
# CONFIG_SUBSYSTEM_ETHERNET_PS7_ETHERNET_0_USE_DHCP is not set
CONFIG_SUBSYSTEM_ETHERNET_PS7_ETHERNET_0_IP_ADDRESS="192.168.10.10"
CONFIG_SUBSYSTEM_ETHERNET_PS7_ETHERNET_0_IP_NETMASK="255.255.255.0"
CONFIG_SUBSYSTEM_ETHERNET_PS7_ETHERNET_0_IP_GATEWAY="192.168.10.1"

#
# Flash Settings
#
CONFIG_SUBSYSTEM_FLASH_PS7_QSPI_0_BANKLESS_SELECT=y
# CONFIG_SUBSYSTEM_FLASH_MANUAL_SELECT is not set
# CONFIG_SUBSYSTEM_FLASH__ADVANCED_AUTOCONFIG is not set

#
# partition 0
#
CONFIG_SUBSYSTEM_FLASH_PS7_QSPI_0_BANKLESS_PART0_NAME="boot"
CONFIG_SUBSYSTEM_FLASH_PS7_QSPI_0_BANKLESS_PART0_SIZE=0x400000

#
# partition 1
#
CONFIG_SUBSYSTEM_FLASH_PS7_QSPI_0_BANKLESS_PART1_NAME="kernel"
CONFIG_SUBSYSTEM_FLASH_PS7_QSPI_0_BANKLESS_PART1_SIZE=0x1400000

#
# partition 2
#
CONFIG_SUBSYSTEM_FLASH_PS7_QSPI_0_BANKLESS_PART2_NAME="bootenv"
CONFIG_SUBSYSTEM_FLASH_PS7_QSPI_0_BANKLESS_PART2_SIZE=0x400000

#
# partition 3
#
CONFIG_SUBSYSTEM_FLASH_PS7_QSPI_0_BANKLESS_PART3_NAME=""
CONFIG_SUBSYSTEM_FLASH_IP_NAME="ps7_qspi_0"

#
# SD/SDIO Settings
#
CONFIG_SUBSYSTEM_PRIMARY_SD_PS7_SD_0_SELECT=y
# CONFIG_SUBSYSTEM_PRIMARY_SD_PS7_SD_1_SELECT is not set
# CONFIG_SUBSYSTEM_PRIMARY_SD_MANUAL_SELECT is not set
CONFIG_SUBSYSTEM_SD_PS7_SD_0_SELECT=y
CONFIG_SUBSYSTEM_SD_PS7_SD_1_SELECT=y

#
# RTC Settings
#
CONFIG_SUBSYSTEM_RTC_MANUAL_SELECT=y
CONFIG_SUBSYSTEM_USB_PS7_USB_0_SELECT=y
CONFIG_SUBSYSTEM_ENDIAN_LITTLE=y

#
# DTG Settings
#
CONFIG_SUBSYSTEM_MACHINE_NAME="template"
CONFIG_SUBSYSTEM_EXTRA_DT_FILES=""

#
# Kernel Bootargs
#
CONFIG_SUBSYSTEM_BOOTARGS_AUTO=y
CONFIG_SUBSYSTEM_BOOTARGS_EARLYPRINTK=y

CONFIG_SUBSYSTEM_DEVICETREE_COMPILER_FLAGS="-@"
# CONFIG_SUBSYSTEM_DTB_OVERLAY is not set
# CONFIG_SUBSYSTEM_REMOVE_PL_DTB is not set
# CONFIG_SUBSYSTEM_ENABLE_NO_ALIAS is not set
# CONFIG_SUBSYSTEM_ENABLE_DT_VERBOSE is not set

#
# FSBL Configuration
#
CONFIG_SUBSYSTEM_FSBL_BSPCOMPILER_FLAGS=""
CONFIG_SUBSYSTEM_FSBL_COMPILER_EXTRA_FLAGS=""

#
# FPGA Manager
#
# CONFIG_SUBSYSTEM_FPGA_MANAGER is not set

#
# u-boot Configuration
#
CONFIG_SUBSYSTEM_UBOOT_CONFIG_TARGET="xilinx_zynq_virt_defconfig"

#
# u-boot script configuration
#
CONFIG_SUBSYSTEM_UBOOT_APPEND_BASEADDR=y
CONFIG_SUBSYSTEM_UBOOT_PRE_BOOTENV=""

#
# JTAG/DDR image offsets
#
CONFIG_SUBSYSTEM_UBOOT_DEVICETREE_OFFSET=0x100000
CONFIG_SUBSYSTEM_UBOOT_KERNEL_OFFSET=0x200000
CONFIG_SUBSYSTEM_UBOOT_RAMDISK_IMAGE_OFFSET=0x4000000
CONFIG_SUBSYSTEM_UBOOT_FIT_IMAGE_OFFSET=0x10000000

#
# QSPI/OSPI image offsets
#
CONFIG_SUBSYSTEM_UBOOT_QSPI_KERNEL_OFFSET=0xA00000
CONFIG_SUBSYSTEM_UBOOT_QSPI_KERNEL_SIZE=0x600000
CONFIG_SUBSYSTEM_UBOOT_QSPI_RAMDISK_OFFSET=0x1000000
CONFIG_SUBSYSTEM_UBOOT_QSPI_RAMDISK_SIZE=0xF80000
CONFIG_SUBSYSTEM_UBOOT_QSPI_FIT_IMAGE_OFFSET=0xA80000
CONFIG_SUBSYSTEM_UBOOT_QSPI_FIT_IMAGE_SIZE=0x1500000

#
# NAND image offsets
#
CONFIG_SUBSYSTEM_UBOOT_NAND_KERNEL_OFFSET=0x1000000
CONFIG_SUBSYSTEM_UBOOT_NAND_KERNEL_SIZE=0x3200000
CONFIG_SUBSYSTEM_UBOOT_NAND_RAMDISK_OFFSET=0x4600000
CONFIG_SUBSYSTEM_UBOOT_NAND_RAMDISK_SIZE=0x3200000
CONFIG_SUBSYSTEM_UBOOT_NAND_FIT_IMAGE_OFFSET=0x1080000
CONFIG_SUBSYSTEM_UBOOT_NAND_FIT_IMAGE_SIZE=0x6400000
CONFIG_SUBSYSTEM_UBOOT_KERNEL_IMAGE="uImage"
CONFIG_SUBSYSTEM_UBOOT_FIT_IMAGE="image.ub"
# CONFIG_SUBSYSTEM_UBOOT_EXT_DTB is not set

#
# Linux Configuration
#
CONFIG_SUBSYSTEM_LINUX_CONFIG_TARGET=""

#
# Image Packaging Configuration
#
# CONFIG_SUBSYSTEM_ROOTFS_INITRAMFS is not set
# CONFIG_SUBSYSTEM_ROOTFS_INITRD is not set
# CONFIG_SUBSYSTEM_ROOTFS_JFFS2 is not set
# CONFIG_SUBSYSTEM_ROOTFS_UBIFS is not set
# CONFIG_SUBSYSTEM_ROOTFS_NFS is not set
CONFIG_SUBSYSTEM_ROOTFS_EXT4=y
# CONFIG_SUBSYSTEM_ROOTFS_OTHER is not set
CONFIG_SUBSYSTEM_SDROOT_DEV="/dev/mmcblk0p2"
CONFIG_SUBSYSTEM_UIMAGE_NAME="image.ub"
CONFIG_SUBSYSTEM_RFS_FORMATS="ext4 tar.gz"
CONFIG_SUBSYSTEM_DTB_PADDING_SIZE=0x1000
# CONFIG_SUBSYSTEM_COPY_TO_TFTPBOOT is not set

#
# Firmware Version Configuration
#
CONFIG_SUBSYSTEM_HOSTNAME="ps-linux"
CONFIG_SUBSYSTEM_PRODUCT="ps-linux"
CONFIG_SUBSYSTEM_FW_VERSION="1.00"

#
# Yocto Settings
#
CONFIG_YOCTO_MACHINE_NAME="zynq-generic"

#
# TMPDIR Location
#
CONFIG_TMP_DIR_LOCATION="${PROOT}/build/tmp"

#
# Devtool Workspace Location
#
CONFIG_DEVTOOL_WORKSPACE_LOCATION="${PROOT}/components/yocto/workspace"

#
# Parallel thread execution
#
CONFIG_YOCTO_BB_NUMBER_THREADS=""
CONFIG_YOCTO_PARALLEL_MAKE=""

#
# Add pre-mirror url 
#
CONFIG_PRE_MIRROR_URL="http://petalinux.xilinx.com/sswreleases/rel-v${PETALINUX_MAJOR_VER}/downloads"

#
# Local sstate feeds settings
#
CONFIG_YOCTO_LOCAL_SSTATE_FEEDS_URL=""
CONFIG_YOCTO_NETWORK_SSTATE_FEEDS=y

#
# Network sstate feeds URL
#
CONFIG_YOCTO_NETWORK_SSTATE_FEEDS_URL="http://petalinux.xilinx.com/sswreleases/rel-v${PETALINUX_MAJOR_VER}/arm/sstate-cache"
# CONFIG_YOCTO_BB_NO_NETWORK is not set
# CONFIG_YOCTO_BUILDTOOLS_EXTENDED is not set

#
# User Layers
#
CONFIG_USER_LAYER_0=""

CONFIG_SUBSYSTEM_BOOTARGS_GENERATED="console=ttyPS0,115200 earlycon root=/dev/mmcblk0p2 rw rootwait"
